Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

## Restore the Default Candidate RP Hold Time

This example restores the default hold time for `VLAN 5` to 0.

- Restore the default RP candidate hold time.

      SEFOS# configure terminal
      SEFOS(config)# interface vlan 5
      SEFOS(pim-comp)# no rp-candidate holdtime

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |