Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Virtual Link

This procedure defines an OSPF virtual link and its related parameters.

1. Type.

       SEFOS# configure terminal
       SEFOS(config)# router ospf

2. Configure the OSPF router ID.

       SEFOS(config-router)# router-id 10.10.2.1

3. Configure the OSPF interface.

       SEFOS(config-router)# network 10.4.0.1 area 0.0.0.0
       SEFOS(config-router)# network 10.10.2.1 area 0.0.0.6

4. Configure the virtual link.

       SEFOS(config-router)# area 0.0.0.6 virtual-link 20.0.0.1 authentication message-digest hello-interval 100 retransmit-interval 100 transmit-delay 50 dead-interval 200 authentication-key asdf

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |