Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure Redistribution

Redistribution configures the protocol from which the routes have to be redistributed into OSPF.

1. Enter Global Configuration mode in SEFOS1.

       SEFOS# configure terminal

2. Enable OSPF globally in SEFOS1.

       SEFOS(config)# router ospf

3. Configure the OSPF router ID.

       SEFOS(config-router)# router-id 10.10.2.1

4. Configure the router as an ASBR router.

       SEFOS(config-router)# asbr router

5. Configure the redistribution of all routes.

       SEFOS(config-router)# redistribute all

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |