Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure SEFOS7

Use the following commands and values to configure the VLAN interfaces in SEFOS7 used in the example topologies presented in this guide (`VLAN 5`).

- Type.

      SEFOS# configure terminal
      SEFOS(config)# interface vlan 5
      SEFOS(config-if)# shut
      SEFOS(config-if)# ipv6 enable
      SEFOS(config-if)# ipv6 address  fec0::3003:0:2/96
      SEFOS(config-if)#  no shut
      SEFOS(config-if)# exit

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |