Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

## Restore the Default BSR-Candidate Value

This example restores the default BSR-candidate value for `VLAN 5` to 0.

- Restore the default BSR preference value.

      SEFOS# configure terminal
      SEFOS(config)# interface vlan 5
      SEFOS(config-if)# no ip pim bsr-candidate
      SEFOS(config-if)# end

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |