Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DHCP Administration Guide

Search Scope:

- This Document
- Entire Library

### DHCP Server

The DHCP server maintains a configured set of IP address pools from which IP addresses are allocated to DHCP clients in the same subnet, whenever they request the server dynamically. Once the IP address is allocated, the server reserves this IP until the lease time for that IP expires. If the client does not renew the IP before the lease time expires, the IP will be returned to the free pool and will be offered to new clients.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |