Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

#### Identifying Chassis Replacement Components

The following table lists the components that are unique to each chassis. When replacing these components, make sure to replace the component that goes with the correct chassis.

Note - For the 7105379 chassis, replace power supply 300-2259 with 7060590 to meet European Union safety requirement EN 60950 2nd Edition +A1.

Component | A90-A | A90-B | A90-D | 7105379
--- | --- | --- | --- | ---
Power supply | 300-1802 | 300-2190 | 300-2259 or 7060590 | 300-2259 or 7060590
Power supply fan tray | 371-2138 | 371-4208 | 371-4653 | 371-4653
Rear fan | 371-1450 | 371-1450 | 371-4753 | 371-4753
CMM | 371-1447 | 371-1447 | 541-4340 or 7019286 | 7045545 or 7068170
Midplane assembly | 541-1983 | 541-3789 | 541-4239 | 7045529
Pass-through NEM1 |  |  |  |
X-Option part number Serviceable item | X4250-N 371-1451 | X4250-N 371-1451 | X4250-N 371-1451 | 7105397 7051003 or 7068169

1Other NEMs are available for each of the chassis models. Refer to the NEM documentation for more details.

Note - If a second part number is listed for a component-chassis combination, this represents the latest part number for that component. Use the second part number when ordering a replacement part.

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |