Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

### Replacing the CMM

You can remove and install a CMM from a powered-off system or from a powered-on system using a hot-swap procedure. The chassis cannot be managed while you replace the CMM hardware.

Note - Make sure that you install the CMM supported for your chassis. For more information, see Identifying Chassis Models and Replacement Components.

This section describes how to remove and install the CMM:

- Remove the CMM

- Install the CMM

- CMM Reset Sequence

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |