Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

## Remove a Power Supply

Before You Begin

| Caution - To ensure proper system cooling and operation, you must replace the power supply within one minute or you must power off the chassis.

1. Press and hold the green button on top of the power supply handle.
2. Rotate the power supply handle away from the power supply and down.
3. Pull the power supply out of the chassis approximately 10 cm (4 inches).
4. While supporting the bottom of the power supply with both hands, pull the power supply all the way out of the chassis.

   | Caution - Remove only one power supply at a time. One power supply must be in the system at all times to supply power to the system.

##### Related Information

- Install a Power Supply

- Remove a FIM

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |