Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

## Install the Fan Board

1. Place the bottom notch on the fan board into the hole in the chassis.
2. Push the top captive screw into place and tighten it.
3. Replace the two rear fan modules that you removed.

   See Replacing a Rear Fan Module.

4. Power on the chassis.

   See Power-On Sequence.

##### Related Information

- Monitoring Faults

- Remove the Fan Board

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |