Skip Navigation Links
Exit Print View
| Oracle Integrated Lights Out Manager (ILOM) 3.x ### Supplement for the Sun Blade 6000 Modular System

Search Scope:

- This Document
- Entire Library

## Display Sensor Readings (CLI)

Note - For ILOM 3.1, replace `/CH` with `/SYSTEM`.

1. Log in to Oracle ILOM CMM.
2. Use the following syntax to display sensor data:

   `show target`

   where target is the path to the sensor. All chassis sensors are located in the `/CH` space.

   The properties describing the sensor are displayed.

   Example:

       -> show /CH/FM3/F0/TACH

        /CH/FM3/F0/TACH
           Targets:

           Properties:
               type = Fan
               ipmi_name = FM3/F0/TACH
               class = Threshold Sensor
               value = 3200.000 RPM
               upper_nonrecov_threshold = N/A
               upper_critical_threshold = N/A
               upper_noncritical_threshold = N/A
               lower_noncritical_threshold = N/A
               lower_critical_threshold = N/A
               lower_nonrecov_threshold = N/A
               alarm_status = cleared

   Note - Alternatively, you can navigate to the target and type the `show` command without any arguments.

Copyright © , 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |