Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

## Reinstall Cables on the Components

For this task, use the cable labels and records that you made as described in Prepare the Chassis for Removal.

- Reinstall cables on the following modular components:

  - CMM connectors

    No. | Description
    --- | ---
    1 | SER MGT – CMM serial management port (RS-232, RJ-45 serial port)
    2 | NET MGT – CMM network management port (Ethernet)

  - NEM connectors

  - PCIe EM connectors

##### Related Information

- Applying Power to the Chassis

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |