Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

## Install a Rear Fan Module

1. Using both hands, align the fan module with the vacant fan module slot.

   Ensure that the green button on the handle of the fan module is at the top of the fan.

2. Slide the fan module into the vacant slot until the front panel meets the chassis.

   After you install the rear fan module, the CMM automatically detects the new module.

##### Related Information

- Monitoring Faults

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |