Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Site Planning Guide

Search Scope:

- This Document
- Entire Library

### Load-Bearing and Handling Precautions

A fully configured Sun Blade 6000 modular system can weigh in excess of 400 pounds (182 kg) while in its shipping container, and 350 pounds (160 kg) when unpacked. Any floor that this system will cross, or surface on which the system is placed, must be able to support these loads.

The system is shipped on a pallet. You must maintain the system in a vertical, upright position while it is in its shipping container. Be sure you use enough personnel when moving the system, especially on sloping loading docks and ramps, to gain access to a raised computer room floor. Move the system slowly and deliberately, and ensure that the floor is free of foreign objects, cables, or other obstructions.

Copyright © 2008, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |