Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

## Repopulate the Chassis

If you depopulated the chassis, follow these steps:

1. Use an antistatic wrist strap.

   Attach this wrist strap to your wrist, and ground the other end of strap to the system chassis.

2. Install the following components.

   Note - Be sure that you replace each component in the same slot that the component was removed from.

   - CMM– SeeInstall the CMM.

   - Rear fan modules – See Install a Rear Fan Module.

   - NEMs – SeeInstall a NEM.

   - PCIe EMs – See Install a PCIe EM.

   - Server/storage modules – See Install a Server or Storage Module.

   - Power supply units – See Install a Power Supply.

   - Filler panels - See Install a Server or Storage Module.

##### Related Information

- Reinstall Cables on the Components

- Depopulate the Chassis

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |