Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Overview

Search Scope:

- This Document
- Entire Library

#### Oracle ILOM CMM

The service processor allows you to manage chassis components and to access the service processors of the individual server modules even when the chassis and/or the server modules are powered off.

Oracle ILOM enables you to:

- Display and configure ILOM network parameters

- Display and configure server module service processor (SP) network parameters

- Connect to the server module SP

- Display the following information about chassis components:

  - Presence of the component

  - FRU ID SEEPROM data

  - Status

In addition to the CMM that manages the chassis, each server module has its own SP that operates independently of the CMM. You can access the server module SP by entering a command on the CMM. They can also be accessed directly, through their SP IP address or through a multi-port adapter on the front of the server module. Some NEMs also have a service processor.

Disk modules do not have a service processor. The CMM provides a limited set of commands for managing them.

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |