Skip Navigation Links
Exit Print View
| Oracle Integrated Lights Out Manager (ILOM) 3.x ### Supplement for the Sun Blade 6000 Modular System

Search Scope:

- This Document
- Entire Library

#### Modular System Oracle ILOM CLI Targets

Oracle ILOM CLI targets represent all software and hardware components and services managed by Oracle ILOM. You specify CLI targets when you interact with Oracle ILOM.

CLI targets are identified by a hierarchal path similar to the directories and files of a file system.

The modular system has three top-level Oracle ILOM CMM targets that are referred to as name spaces. The following table shows the CLI targets for Oracle ILOM 3.0 and 3.1.

ILOM 3.0 target | ILOM 3.1 target | Description
--- | --- | ---
/CMM | /CMM | Use this target to configure Oracle ILOM CMM attributes for such things as alerts, clients, the Oracle ILOM clock, network addresses, and users.
/CH | /System | Provides component inventory, environmental status, and hardware management at the chassis level. The sub-targets under `/CH` or `/System` correspond to names of the installed hardware components.
/STORAGE | /STORAGE | Used to manage chassis storage (storage on storage blades). Chassis storage can be assigned to blade servers in the chassis.

Each target has a set of properties. Properties are the configurable attributes specific to each target.

Note - There are additional targets for server modules. For further information on Oracle ILOM CLI targets, see Oracle ILOM Documentation.

Copyright © , 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |