Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Site Planning Guide

Search Scope:

- This Document
- Entire Library

### Compatible Cabinets

The chassis is designed for rackmounting. It can be mounted into 19-inch EIA-310D cabinets with a depth of 35.4 to 39.4 inches (90.0 to 100.1 cm). The chassis can accommodate corresponding front-to-back, rail-to-rail spacing of 26.77 inches (68.0 cm) to 34.25 inches (87.0 cm).

Oracle offers EIA 310D-compliant cabinets for mounting the Sun Blade 6000 modular system. The Sun Rack 1000 cabinet family is among the newer cabinets from Oracle. These cabinets are designed to hold three Sun Blade 6000 modular system (Sun Rack 1000-38) or four Sun Blade 6000 modular systems (Sun Rack 1000-42). The following table lists the physical specifications for the Sun Rack 1000 cabinets.

Specification | Sun Rack 1000-38 | Sun Rack 1000-42
--- | --- | ---
Usable rack units | 38 | 42
Height | 74 inches (188 cm) | 81 inches (205.7 cm)
Width | 23.5 inches (60 cm) | 23.5 inches (60 cm)
Depth | 39.4 inches (1000 cm) | 39.4 inches (1000 cm)
Weight of empty rack | 370 lb (167.8 kg) | 426 lb (193.2 kg)
Weight of empty rack with shipping pallet | 540 lb (244.9 kg) | 683 lb (309.7 kg)
Weight of empty rack with MPS (no pallet) | 465 lb (210.9 kg) | 521 lb (236.3 kg)
Load capacity | 1200 lb (544 kg) | 1200 lb (544 kg)

Copyright © 2008, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |