Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Site Planning Guide

Search Scope:

- This Document
- Entire Library

### Number of Chassis Supported in a Rack

Up to four Sun Blade 6000 chassis can be installed in a 1000-42 rack, with the exceptions shown in the following list.

The following configurations are supported by MPS:

- Worst case consumption (32A), 60A-3 phase: one Sun Blade 6000 chassis

- One 32A-3 phase – three Sun Blade 6000 chassis

- Two 60A-3 phase – three Sun Blade 6000 chassis

- Two 30A-1 phase – one Sun Blade 6000 chassis

Copyright © 2008, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |