Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

#### PCIe EM Service Overview

A pair of PCIe EMs is assigned to each server module in the chassis. All PCIe EMs connect to a chassis midplane. The midplane provides an interconnect between the server modules and the PCIe EMs installed in the chassis. The midplane connections between the server module and the PCI EM are logically defined by the midplane.

If the amber Service Action Required indicator on a PCIe EM is lit, this indicates a problem with the PCIe EM.

##### Related Information

- Remove a PCIe EM

- Install a PCIe EM

- Monitoring Faults

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |