Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

## Remove the Chassis From the Rack

| Caution - The chassis is heavy. Use a mechanical lift, or depopulate the chassis and use four people to lift the chassis.

1. Remove two upper rear brackets from the rack by removing four screws that secure the bracket.
2. Remove the eight screws that secure the front of the chassis to the rack.
3. From the front of the rack, slowly pull the chassis forward a few inches.
4. Remove the chassis the rest of the way using a mechanical lift, or manually, using four people.
5. Set the chassis on a sturdy surface.

##### Related Information

- Reinstalling the Chassis Into a Rack

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |