Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

## Remove the Fan Board

1. Power off the chassis.

   Refer to the server module documentation, and see Power Off the Chassis.

2. Remove the two rear fan modules that are in front of the fan board that you want to remove.

   See Replacing a Rear Fan Module.

3. Loosen the captive screw on the fan board until you can pull the top of the board forward.

   This screw needs to be fully unscrewed because the screw disengages the fan board connector from the midplane.

4. Lift the board up and off the chassis.

##### Related Information

- Install the Fan Board

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |