Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

## View Component Status Using the Oracle ILOM CLI

You can monitor chassis and component faults from the Oracle ILOM CLI.

1. Log into the Oracle ILOM CLI.
2. Type the appropriate `show` command to display information about system components.

   For example, if the power supply AC-1 LED is lit, you would type the following command:

       -> show /CH/PS0/S1/V_12V_ERR

       /CH/PS0/S1/V_12V_ERR
       Targets:

       Properties:
        type = Voltage
        ipmi_name = PS0/S1/V_12V_ERR
        class = Discrete Sensor
        value = Predictive Failure Asserted
        alarm_status = cleared

       Commands:
        cd
        show

   In the example, `value = Predictive Failure Asserted` shows a 12-volt rail issue, which most likely means a faulty power supply unit.

   Refer to the sensor information in Oracle ILOM 3.0 Supplement for the Sun Blade 6000 Modular Systems for more information about reading the sensors to determine fault information.

##### Related Information

- View Component Status Using Oracle ILOM Web Interface

- Monitor Faults With the Oracle ILOM CLI Event Log

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |