Skip Navigation Links
Exit Print View
| Oracle Integrated Lights Out Manager (ILOM) 3.x ### Supplement for the Sun Blade 6000 Modular System

Search Scope:

- This Document
- Entire Library

#### Server Module Sensors in Oracle ILOM 3.0

The following tables lists possible sensors for server modules. Not all server modules have all sensors.

Sensor | Reading | State | Event | Description
--- | --- | --- | --- | ---
`BLn/PRSNT` | `0x0001` | Device Absent | No | Server module is not present.
| `0x0002` | State Present | No | Server module is present.
`BLn/STATE` | `0x0001` | Running | No | Server module is running.
| `0x0004` | Power Off | No | Server module is not powered off.
| `0x0020` | Off Duty | No | Server module is ready to remove.
`BLn/ERR` | `0x0001` | Predictive Failure Asserted | Yes | Server module has failed.
| `0x0002` | Predictive Failure Deasserted | Yes | Server module has not failed.
`BLn/VPS` | n/a | n/a | n/a | Reports the virtual power for the server modules.

##### Related Information

- Display Sensor Readings (CLI)

- Chassis Sensors in Oracle ILOM 3.0

- Fan Sensors in Oracle ILOM 3.0

- Power Supply Sensors in Oracle ILOM 3.0

- NEM Sensors in Oracle ILOM 3.0

- Sensor Types

Copyright © , 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |