Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

## Remove a FIM

Before You Begin

| Caution - To ensure proper system cooling and operation, you must replace the power supply within one minute or you must power off the chassis.

1. Remove power supply 0 from the chassis.

   See Remove a Power Supply.

2. Push back the power supply air baffle.
3. Press the button on the right side of the FIM.
4. Remove the FIM from the chassis.

##### Related Information

- Install a FIM

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |