Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

### Powering Off the System and Components

See the guidelines for powering off the system and components in the following table:

If you are removing | Then follow these procedures
--- | ---
Server or storage modules | Power Off the Server Modules and Storage Modules
Midplane, internal power cables, or fan boards | Power Off the Chassis
Power supplies, fan modules, FIM, CMM, PCIe EMs, or NEMs | Most of these modules do not require the chassis to be powered off before being replaced. However, certain NEMs do require the chassis to be powered off. Check the NEM documentation for more information.

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |