Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

## Install a FIM

1. Align the FIM with the FIM slot.
2. Slide the FIM into the FIM slot.
3. Reinstall power supply 0 into the chassis.

   See Remove a Server or Storage Module.

##### Related Information

- Remove a FIM

- Monitoring Faults

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |