Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Overview

Search Scope:

- This Document
- Entire Library

### PCIe EMs

The PCIe EMs are designed to offer independent, dedicated I/O functions configurable on a per server module basis.

Each blade slot has two dedicated PCIe EM slots, numbered as follows that correspond to the server modules as shown in the following diagram.

The following table describes how the blade slots correspond to the PCIe EM slots.

Blade Slot | PCIe EM Slots
--- | ---
0 | 0.0, 0.1
1 | 1.0, 1.1
2 | 2.0, 2.1
3 | 3.0, 3.1
4 | 4.0, 4.1
5 | 5.0, 5.1
6 | 6.0, 6.1
7 | 7.0, 7.1
8 | 8.0, 8.1
9 | 9.0, 9.1

The PCIe EM format is a standard developed by the PCI-SIG standards organization. The chassis midplane implements PCI Express connectivity between the PCIe EMs and server modules and assigns two PCIe EMs to each server module. All PCIe EMs are hot-pluggable, allowing system administrators to easily replace them.

PCIe EMs can be installed in a system without any modification to the connected server module hardware. The Sun Blade 6000 modular system supports industry-standard, hot-swappable PCIe EMs.

The following table shows the supported PCIe EMs and links to available PCIe EM documentation. The PCIe EMs listed here were available at the time this document was last updated.

PCIe EM | Product Number | Document URL
--- | --- | ---
Ethernet PCIe EMs
Sun PCI Express Dual Gigabit Ethernet MMF/UTP ExpressModule | X7283A | http://download.oracle.com/docs/cd/E19380-01/index.html
Sun x4 PCIe Quad Gigabit Ethernet ExpressModule | X7284A | http://download.oracle.com/docs/cd/E19640-01/index.html
Sun Quad GbE UTP x8 PCIe ExpressModule | X7287A | http://docs.oracle.com/cd/E19113-01/
Sun Dual 10GbE SFP+ PCIe ExpressModule | X1108A | http://download.oracle.com/docs/cd/E19571-01/index.html
Sun Dual 10GbE SFP+ PCIe 2.0 ExpressModule | X1110A | http://download.oracle.com/docs/cd/E19254-01/index.html
Sun Dual 10GbE XFP PCIe ExpressModule | X1028A | http://download.oracle.com/docs/cd/E19862-01/index.html
Host Bus Adapter PCIe EMs
Sun StorageTek 4 Gb Fibre Channel ExpressModule HBA (Qlogic) | SG-XPCIE2FC-QB4-Z | http://download.oracle.com/docs/cd/E19419-01/index.html
Sun StorageTek 4 Gb Fibre Channel ExpressModule HBA (Emulex) | SG-XPCIE2FC-EB4-Z | http://download.oracle.com/docs/cd/E19919-01/index.html
Sun StorageTek Dual 8Gb Fibre Channel Dual GbE ExpressModule HBA (Qlogic) | SG-XPCIEFCGBE-Q8-Z | http://download.oracle.com/docs/cd/E19925-01/index.html
Sun StorageTek Dual 8Gb Fibre Channel Dual GbE ExpressModule HBA (Emulex) | SG-XPCIEFCGBE-E8-Z | http://download.oracle.com/docs/cd/E19353-01/index.html
Sun StorageTek Dual 4 Gb FC Dual GbE HBA ExpressModule (Qlogic) | SG-XPCIE2FCGBE-Q-Z | http://download.oracle.com/docs/cd/E19883-01/index.html
Sun StorageTek Dual 4 Gb FC Dual GbE HBA ExpressModule (Emulex) | SG-XPCIE2FCGBE-E-Z | http://download.oracle.com/docs/cd/E19732-01/index.html

Copyright © 2009, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |