Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### Acoustic Noise Emissions

Declared noise emissions for the SPARC T4-1 server are in accordance with ISO 9296 standards.

Table 5 Acoustic Noise Emissions for the SPARC T4-1 Server

Description | Parameter | Value
--- | --- | ---
LwAd | Operating acoustic noise (max.) Idling acoustic noise | 8.5 B1 7.1 B
LwAm (bystander positions) | Operating acoustic noise (max.) Idling acoustic noise | 70.1 dB 59.3 dB

11 B = 10 dB

##### Related Information

- SPARC T4-1 Server Safety and Compliance Guide

- Environmental Specifications

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |