Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

### Powering On the Server for the First Time

These topics provide instructions for booting Oracle's SPARC T4-1 server for the first time and for enabling the NET MGT port. It consists of the following topics:

Step | Description | Links
--- | --- | ---
1. | Review the behavior of Oracle ILOM console output when the system is powered on the first time. | Oracle ILOM System Console
2. | Connect the server to a terminal display. | Connect a Terminal or Emulator to the SER MGT Port
3. | Power on the server. | Power On the Server for the First Time
4. | Check that the server is operational. | Verify Functionality
5. | (Optional) Assign a static IP address to the SP. | Assigning a Static IP Address to the SP
6. | Review the Oracle Solaris OS configuration parameter descriptions. | Oracle Solaris OS Configuration Parameters

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |