Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Display FRU Information (`show` Command)

- At the Oracle ILOM prompt, type the `show` command.

  In the following example, the `show` command displays information about a DIMM.

      -> show /SYS/MB/CMP0/B0B0/CH0/D0

      /SYS/MB/CMP0/B0B0/CH0/D0
         Targets:
             T_AMB
             SERVICE

         Properties:
             Type = DIMM
             ipmi_name = B0/C0/D0
             component_state = Enabled
             fru_name = 2048MB DDR3 SDRAM
             fru_description = DDR3 DIMM 2048 Mbytes
             fru_manufacturer = Samsung
             fru_version = 0
             fru_part_number = ****************
             fru_serial_number = ******************
             fault_state = OK
             clear_fault_action = (none)

         Commands:
             cd
             set
             show

##### Related Information

- Oracle ILOM 3.0 documentation

- Oracle ILOM Troubleshooting Overview

- Access the SP (Oracle ILOM)

- Check for Faults (`show` `faulty` Command)

- Check for Faults (`fmadm` `faulty` Command)

- Clear Faults (`clear_fault_action` Property)

- Service-Related Oracle ILOM Commands

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |