Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### POST-Detected Fault Example (`show` `faulty` Command)

The following is an example of the `show` `faulty` command displaying a fault that was detected by POST. These kinds of faults are identified by the message `Forced` `fail` reason, where reason is the name of the power-on routine that detected the fault.

    -> show faulty
    Target              | Property               | Value
    --------------------+------------------------+--------------------------------
    /SP/faultmgmt/0     | fru                    | /SYS/PM0/CMP0/B0B0/CH0/D0
    /SP/faultmgmt/0     | timestamp              | Oct 12 16:40:56
    /SP/faultmgmt/0/    | timestamp              | Oct 12 16:40:56
    faults/0            |                        |
    /SP/faultmgmt/0/    | sp_detected_fault      | /SYS/PM0/CMP0/B0B0/CH0/D0
    faults/0            |                        | Forced fail(POST)

##### Related Information

- No Faults Detected Example (`show` `faulty` Command)

- Power Supply Fault Example (`show` `faulty``` Command)

- Power Supply Fault Example (`fmadm` `faulty` Command)

- PSH-Detected Fault Example (`show` `faulty` Command)

- Service-Related Oracle ILOM Commands

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |