Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

#### Server Overview

This topic provides a high-level introduction to the main components and capabilities of the server.

Figure 1 Oracle's SPARC T4-1 Server

Component | Description
--- | ---
Chassis | Rack-mountable server with a 2RU form-factor.
CPU | One T4 2.85 GHz multicore processor.
Memory | Sixteen DDR3 DIMM memory slots supporting 4, 8, or 16 GB modules.
Storage devices | For internal storage, the server provides: Eight 2.5-inch drive bays, accessible through the front panel. A slot-loading DVD+/-RW drive on front panel.
USB ports | Four external USB 2.0 ports (two each on the front and rear panels).
Video ports | One high-density DB-15 video port (rear panel).
PCI Express 2.0 I/O slots | Six standard half-length, low-profile PCIe 2.0 slots. Two of the six slots are capable of accepting either a PCIe card or a XAUI card.
Ethernet ports | Four 10/100/1000 Mbps, RJ-45-based, autonegotiating Ethernet ports (rear panel).
SP | Oracle Integrated Lights Out Manager (ILOM) with RJ-45 serial and Ethernet interfaces.
Power supplies | Two hot-swappable power supplies
Cooling fans | Six sets (N+1) of hot-swappable counter-rotating fan modules.

##### Related Information

- SPARC T4-1 Server Service Manual

- Oracle ILOM documentation

- Front Panel Components

- Front Panel System LEDs and Buttons

- Rear Panel Components

- Rear Panel System LED and Button

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |