Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

#### Rear Components

The following figure shows the layout of the I/O ports, PCIe ports, 10 Gbit Ethernet (XAUI) ports (if equipped) and power supplies on the rear panel.

Figure 31 Rear Panel Components and Indicators

Figure Legend

1 Power supply 0

2 Power supply 1

3 Locator LED button

4 Service Required LED

5 Power OK LED

6 Service processor SER MGT port

7 Service processor NET MGT port

8 Gbit Enet port NET0

9 Gbit Enet port NET1

10 Gbit Enet port NET2

11 Gbit Enet port NET3

12 Access hole for physical presence button

13 USB port 0

14 USB port 1

15 VGA video port

16 PCIe slot 3 or XAUI slot 1

17 PCIe slot 0 or XAUI slot 0

18 PCIe slot 4

19 PCIe slot 1

20 PCIe slot 5

21 PCIe slot 2

##### Related Information

- Front Components

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |