Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### Hot Service, Replaceable by Customer

The following table identifies the components that can be replaced while power is present on the server. These components can be replaced by customers.

Hot Service Components (system can have power present) | Notes
--- | ---
Hard disk drive (HDD) | Drive must be offline
HDD filler | Needed to preserve proper interior air flow
Power supply | If two power supplies are in use
Fan module |

Although hot service procedures can be performed while the server is running, you should usually bring it to standby mode as the first step in the replacement procedure. Refer to Power Off the Server (Power Button - Graceful) for instructions.

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |