Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### SER MGT Port

The SER MGT RJ-45 port, located on the rear panel, provides the default connection to the system console.

Figure 21 SER MGT Port

Figure Legend

1 Clear to Send

2 Data Carrier Detect

3 Transmit Data

4 Ground

5 Ground

6 Receive Data

7 Data Terminal Ready

8 Ready to Send

##### Related Information

- Front Panel Components

- Rear Panel Components

- Connect the SER MGT Port Cable

- Connect a Terminal or Emulator to the SER MGT Port

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |