Skip Navigation Links
Exit Print View
| SPARC T4-1 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Clear Faults (`clear_fault_action` Property)

Use the `clear_fault_action` property of a FRU with the `set` command to manually clear Oracle ILOM-detected faults from the SP.

If Oracle ILOM detects a FRU replacement, Oracle ILOM automatically clears the fault. For PSH-diagnosed faults, if the replacement of the FRU is detected by the system or you manually clear the fault on the host, the fault is also cleared from the SP. In such cases, you do note need to clear the fault manually.

Note - For PSH-detected faults, this procedure clears the fault from the SP but not from the host. If the fault persists in the host, clear the fault manually as described in Clear PSH-Detected Faults.

- At the Oracle ILOM prompt, use the `set` command with the `clear_fault_action=True` property.

  This example begins with an excerpt from the `fmadm` `faulty` command showing power supply 0 with a voltage failure. After the fault condition is corrected (a new power supply has been installed), the fault state is cleared.

  Note - In this example, the characters SPT at the beginning of the message ID indicate that the fault was detected by Oracle ILOM.

      [...]

      faultmgmtsp> fmadm faulty
      ------------------- ------------------------------------ ------------ -------
      Time                UUID                                 msgid        Severity
      ------------------- ------------------------------------ ------------ -------
      2010-08-11/14:54:23 ********-****-****-****-************ SPT-8000-LC  Critical

      Fault class : fault.chassis.power.volt-fail

      Description : A Power Supply voltage level has exceeded acceptible limits.

      [...]

      -> set /SYS/PS0 clear_fault_action=true
      Are you sure you want to clear /SYS/PS0 (y/n)? y

      -> show

       /SYS/PS0
          Targets:
              VINOK
              PWROK
              CUR_FAULT
              VOLT_FAULT
              FAN_FAULT
              TEMP_FAULT
              V_IN
              I_IN
              V_OUT
              I_OUT
              INPUT_POWER
              OUTPUT_POWER
          Properties:
              type = Power Supply
              ipmi_name = PSO
              fru_name = /SYS/PSO
              fru_description = Powersupply
              fru_manufacturer = Delta Electronics
              fru_version = 03
              fru_part_number = *******
              fru_serial_number = ******
              fault_state = OK
              clear_fault_action = (none)

          Commands:
              cd
              set
              show

##### Related Information

- Oracle ILOM Troubleshooting Overview

- Access the SP (Oracle ILOM)

- Display FRU Information (`show` Command)

- Check for Faults (`show` `faulty` Command)

- Check for Faults (`fmadm` `faulty` Command)

- Service-Related Oracle ILOM Commands

Copyright © 2011, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |