Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

#### Handling Precautions

| Caution - Deploy the anti-tilt bar on the equipment rack before beginning an installation.

| Caution - Always load equipment into a rack from the bottom up so that it will not become top-heavy and tip over.

| Caution - A fully configured SPARC T4-4 server weighs approximately 175 lb. (79 kg). An equipment lift is required to lift and mount this server into a rack enclosure when using the procedures in this document.

| Caution - Always communicate your intentions clearly before, during, and after each step of the rackmounting procedure to minimize confusion.

##### Related Information

- ESD Precautions

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |