Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### NET MGT Port

The NET MGT port is an RJ-45 connector located on the system back panel. This port must be configured prior to use.

Pin | Signal Description | Pin | Signal Description
--- | --- | --- | ---
1 | Transmit Data + | 5 | Common Mode Termination
2 | Transmit Data – | 6 | Receive Data –
3 | Receive Data + | 7 | Common Mode Termination
4 | Common Mode Termination | 8 | Common Mode Termination

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |