Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

### Installing the Server

These topics describe how to install the server into an equipment cabinet equipped with square mounting holes. If you are installing the server into a cabinet equipped with round mounting holes, see Determine Correct Rackmount Hardware.

Note - If your rackmount kit came with its own instructions, use the instructions in your rackmount kit instead of the instructions in this chapter. After performing the server installation, proceed to Powering On the Server for the First Time for first-time power on.

If you are shipping the equipment rack to another location for final installation, or installing the server into a vehicle, install the shipping bracket assembly. See Installing the Shipping Bracket Assembly (Optional).

Step | Description | Links
--- | --- | ---
1 | Install optional components. | Install Optional Components
2 | Ensure that your rack is compatible with the server requirements. | Rack Compatibility
3 | Determine the correct rackmounting hardware and install the hardware. | Determine Correct Rackmount Hardware Mark the Rackmounting Location Install the Rackmount Hardware
4 | Install the server in the rack. | Install the Server
5 | If you are installing the server into a vehicle or into a rack that will be shipped to another location, install the Shipping Bracket Assembly. | Installing the Shipping Bracket Assembly (Optional)
6 | (Optional) Install the CMA. | Installing the CMA (Optional)
7 | Review cabling requirements and port information. Attach data and management cables to the server. | Connecting the Server Cables
8 | Configure the Oracle ILOM SP and power on the server for the first time. | Powering On the Server for the First Time

##### Related Information

- Confirming Server and Site Specifications

- Installing the Server

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |