Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

#### Hard Drive LEDs

The status of each drive is represented by the same three LEDs.

Table 23 Status LEDs for Hard Drives

No. | LED | Icon | Description
--- | --- | --- | ---
1 | Ready to Remove (blue) |  | Indicates that a drive can be removed during a hot-plug operation.
2 | Service Required (amber) |  | Indicates that the drive has experienced a fault condition.
3 | OK/Activity (green) |  | Indicates the drive's availability for use. On – Read or write activity is in progress. Off – Drive is idle and available for use.

##### Related Information

- Hard Drive Hot-Pluggable Capabilities

- Hard Drive Configuration Reference

- Locate a Faulty Hard Drive

- Remove a Hard Drive

- Install a Hard Drive

- Verify Hard Drive Functionality

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |