Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

#### Service Processor Card Overview

If the service processor card is replaced, the configuration settings maintained in the service processor card will need to be restored. Before replacing the service processor card, you should save the configuration using the Oracle ILOM backup utility.

System firmware consists of both SP and host components. The SP component is located on the service processor card and the host component is located on the host. These two components must be compatible. When the service processor card is replaced, the SP firmware component on the new service processor card may be incompatible with the existing host firmware component. In this case, the system firmware must be loaded as described in Install the Service Processor Card.

##### Related Information

- Locate a Faulty Service Processor Card

- Remove the Service Processor Card

- Install the Service Processor Card

- Verify Service Processor Card Functionality

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |