Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Remove a Fan Module

The fan module is a hot-service component that can be replaced by a customer.

1. Locate the faulty fan module that you want to remove from the server.
   - See Rear Panel Components for the locations of the fan modules in the server.
   - See Locate a Faulty Fan Module to locate a faulty fan module.
2. Determine if you can remove the fan module with the server running or not.

   See Fan Module Overview to determine if you can remove a fan module with the server running or if you must shut down the server before removing a fan module.

   - If you can remove a fan module with the server running, go to Step 3.

   - If you cannot remove a fan module with the server running, see Removing Power From the Server to power down the server before continuing.

3. Press down on the middle portion of the fan lever and lower the lever slightly to disengage the fan latch.
4. Lower the fan lever completely and pull out on the fan module to remove the fan module from the server.

##### Related Information

- Fan Module Overview

- Fan Module Configuration Reference

- Fan Module LED

- Locate a Faulty Fan Module

- Install a Fan Module

- Verify Fan Module Functionality

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |