Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Remove the System Configuration PROM

The system configuration PROM is a cold-service component that can be replaced only by authorized service personnel.

Before beginning this procedure, ensure that you are familiar with the cautions and safety instructions described in Safety Information.

| Caution - This procedure involves handling circuit boards that are extremely sensitive to static electricity. Ensure that you follow ESD preventative practices to avoid damaging the circuit boards.

Note - The System Configuration PROM is plugged into a socket on the motherboard. It includes a yellow barcode label.

1. Remove the main module from the server.

   See Remove the Main Module.

2. Take the necessary ESD precautions.

   See Prevent ESD Damage.

3. Locate the system configuration PROM on the main module.

   See Main Module Components.

4. Grasp the system configuration PROM and lift it up to remove it from the main module.

##### Related Information

- System Configuration PROM Overview

- Install the System Configuration PROM

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |