Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

##### Cold Service, Replacement by Customer

The following components require the server to be powered down. These components can be replaced by customers.

Cold Service (power down server and unplug power cables) | Notes
--- | ---
Processor module |
DIMM |
Main module |
System battery |
RAID expansion module |
Service processor card |
Rear I/O module |

See Power Off the Server (SP Command) for the procedure to shut down the server.

##### Related Information

- Removing Power From the Server

- Accessing Internal Components

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |