Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install a Fan Module

1. Insert the fan module into the empty fan module slot.
2. Lift the fan lever up completely until the latch clicks into place to completely seat the fan module into the slot.
3. Power on the server, if necessary.

   If you had to power off the server before removing and installing a new fan, see Returning the Server to Operation to power on the server again.

4. Verify the fan module functionality.

   See Verify Fan Module Functionality.

##### Related Information

- Fan Module Overview

- Fan Module Configuration Reference

- Fan Module LED

- Locate a Faulty Fan Module

- Remove a Fan Module

- Verify Fan Module Functionality

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |