Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Remove the Front Shipping Bracket

Remove the front shipping bracket after the server cabinet reaches its final destination.

1. Remove the two short No. 2 Phillips screws that are stored with the shipping bracket.
2. Remove the two screws that secure the front shipping bracket to the cabinet.
3. Slide the front shipping bracket out from the front of the cabinet.
4. Install the two short No. 2 Phillips screws into the lower two front panel screws.

   Use the screws that were stored in the front shipping bracket during transit.

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |