Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

## Install the Service Processor Card

1. Lower the side of the service processor card with the `Align Tab` sticker down on the service processor tab on the motherboard.
2. Lower the other side of the service processor card down and press down on the service processor card to seat it into the connectors on the motherboard.
3. Install the main module back into the server.

   See Install the Main Module.

4. Connect a terminal or a terminal emulator (PC or workstation) to the serial management port.

   If the replacement service processor card detects that the SP firmware is not compatible with the existing host firmware, further action will be suspended and the following message will be delivered over the serial management port.

       Unrecognized Chassis: This module is installed in an unknown or
       unsupported chassis. You must upgrade the firmware to a newer
       version that supports this chassis.

   If you see this message, go on to Step 5.

5. Download the system firmware.
   1. Configure the service processor card's network port to enable the firmware image to be downloaded.

      Refer to the Oracle ILOM documentation for network configuration instructions.

   2. Download the system firmware.

      Follow the firmware download instructions in the Oracle ILOM documentation.

      Note - You can load any supported system firmware version, including the firmware revision that had been installed prior to the replacement of the service processor card.

6. Restore the SP configuration information that you backed up earlier.

   At the Oracle ILOM prompt, type:

       -> cd /SP/config
       -> load -source uri target

   where:

   - The acceptable values for uri are:
     - tftp
     - ftp
     - sftp
     - scp
     - http
     - https
   - target is the remote location where you stored the configuration information.

     For example:

         -> load -source tftp://129.99.99.99/pathname

7. Verify the SP.

   See Verify Service Processor Card Functionality.

##### Related Information

- Service Processor Card Overview

- Locate a Faulty Service Processor Card

- Remove the Service Processor Card

- Verify Service Processor Card Functionality

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |