Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

#### Fan Module Overview

The server will continue to operate at full capacity with four or more fan modules installed in the server. The server will not operate with fewer than four fan modules installed and operating. If the server is operating with four fan modules installed and one or more of those four fan modules fails, the server will power down to keep from overheating. You can perform a hot-service on a fan module only if four or more fan modules are operational.

##### Related Information

- Fan Module Configuration Reference

- Fan Module LED

- Locate a Faulty Fan Module

- Remove a Fan Module

- Install a Fan Module

- Verify Fan Module Functionality

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |