Skip Navigation Links
Exit Print View
| SPARC T4-4 Server HTML Document Collection

Search Scope:

- This Document
- Entire Library

#### Fan Module LED

Figure 27 Fan Module LED

Table 26 Fan Module Status LEDs

No. | LED | Icon | Description
--- | --- | --- | ---
1 | Service Required (amber) |  | The LED amber when the fan module is faulty. The server Fan Fault LED is also lit when a Fan module LED is amber.

The front and rear panel Service Required LEDs also turn on if the server detects a fan module fault.

If the fan fault causes an overtemperature condition to occur, the server Overtemp LED will turn on, and an error message will be logged and displayed on the system console.

##### Related Information

- Fan Module Overview

- Fan Module Configuration Reference

- Locate a Faulty Fan Module

- Remove a Fan Module

- Install a Fan Module

- Verify Fan Module Functionality

Copyright © 2011, 2014, Oracle and/or its affiliates. All rights reserved. Legal Notices |